M10 CEMENT BASED LEVELING / WEARING SCREEDS

To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

140 PROPRIETARY POLYMER MODIFIED LEVELLING SCREEDS

* Substrate : …………………
* Screed manufacturer : RIW Limited, Arc House, Terrace Road South, Binfield,

RG42 4PZ.

Tel : 01344 397777 Fax : 01344 862010

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk) Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementfill FC

* Screed construction : Fullybonded.
* Thickness :

- Nominal : 3mm.

- Minimum : 0mm.

- Maximum : 6mm per layer.

* Mix :

- Proportions : 6. 5 parts powder to 1 part water, by volume.

* Primer : RIW Cementseal Primer
* Finish : …………………

- To receive …………………

- Other requirements …………………