C42 REPAIRING / RENOVATING / CONSERVING CONCRETE

 To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

310A REPAIR MORTAR

* Type : Polymer modified cementitious mortar
* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

 Tel : +44 1753 944200

 E-mail : technical@riw.co.uk

 Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementfill FC

* Application thickness : 6mm maximum per layer.
* Primer : Not required

*or : for highly porous substrates*

* Primer : RIW Cementseal Primer

J40/310333333333

3100110101010293I8E4844444

320A LEVELLING / SMOOTHING COATS

* Type : Polymer modified cementitious mortar
* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

 Tel : +44 1753 944200

 E-mail : technical@riw.co.uk

 Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementfill FC

* Application thickness : 0 to 6mm.
* Primer : Not required

*or : for highly porous substrates*

* Primer : RIW Cementseal Primer