C42 REPAIRING / RENOVATING / CONSERVING CONCRETE

To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

310A REPAIR MORTAR

* Type : Modified polymer rich cementitious coating
* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementflex

* Number of coats : Two
* Thickness per coat : 1mm vertical
* Primer : Not required.

*or : for horizontal surfaces*

* Number of coats : One
* Thickness per coat : 2mm
* Primer : RIW Cementseal Primer.