C42 REPAIRING / RENOVATING / CONSERVING CONCRETE

To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

310A REPAIR MORTAR

* Type : Copolymer cementitious mortar
* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Cementfill HB

* Application thickness : 5mm minimum, 80mm maximum per layer.
* Primer : Not required

*or : for highly porous substrates*

* Primer : RIW Cementseal Primer