F30 ACCESSORIES / SUNDRY ITEMS FOR BRICK / BLOCK / STONE WALLING

 To be read with Preliminaries / General conditions.

 FLEXIBLE DAMP PROOF COURSES / CAVITY TRAYS

F30/330 DAMP PROOF COURSE – POLYMERIC.

* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

 Tel : +44 1753 944200

 E-mail : technical@riw.co.uk

 Web : [www.riw.co.uk](http://www.riw.co.uk)

 - Product reference : RIW Sheetseal 9000 DPC.

 INSTALLATION OF DPC’s / CAVITY TRAYS

F30/415 HORIZONTAL DPC’s

* Placement : In continuous lengths on full even bed of fresh mortar, with 100mm laps at joints and full laps at angles.
* Width : At least full width of leaf unless otherwise specified.

Edges of DPC not covered with mortar or projecting into cavity.

* Overlying construction : Immediately cover with full even bed of mortar to receive next masonry course.
* Overall finished joint thickness : As close to normal as practicable.

F30/425 GROUND LEVEL DPC’s

* Joint with damp proof membrane : Continuous and effectively sealed.

F30/435 STEPPED DPC’s IN EXTERNAL WALLS

* External walls on sloping ground : Install DPC’s not less than 150mm above adjoining finished ground level.

465 SEALING DPC’s …………………

* Overlaps and junctions : Seal with RIW Jointing Tape.