F30 ACCESSORIES / SUNDRY ITEMS FOR BRICK / BLOCK / STONE WALLING

To be read with Preliminaries / General conditions.

FLEXIBLE DAMP PROOF COURSES / CAVITY TRAYS

F30/370 PREFORMED CAVITY TRAYS

* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product references and locations : RIW Sheetseal 9000 DPC

* + Column Cloak Cavity Tray.
  + Bullseye Window Cavity Tray.
  + Arch - window Cavity Tray.
* Placement : To provide a free draining and watertight installation.

F30/380 PREFORMED DPC / CAVITY TRAY JUNCTION CLOAKS / STOP ENDS

* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

* Product references and locations : RIW Sheetseal 9000 DPC
* Full Height, RH stop end unit.
* Full Height, LH stop end unit.
* 75mm high (sloping), RH stop end unit.
* 75mm high (sloping), LH stop end unit.
* Corner unit.
* 75mm step multi hand change level unit.
* 150mm step multi hand change level unit.
* 225mm step multi hand change level unit.
* Placement : To provide a free draining and watertight installation. Seal laps with DPC’s and / or cavity trays.

F30/385 PREFORMED DPC / CAVITY TRAY JUNCTION CLOAKS / STOP ENDS

* Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product references and locations : As shown on drawings.

* Placement: Seal laps with DPC’s and / or cavity trays.