J40 FLEXIBLE SHEET TANKING / DAMP PROOFING

To be read with Preliminaries / General conditions.

TYPES OF TANKING / DAMP PROOFING

J40/290 HIGH DENSITY POLYETHYLENE / POLYPROPYLENE STUDDED DAMP PROOFING

* Substrate : …………………

- Preparation : In accordance with manufacturer’s recommendations.

* Manufacturer : RIW Limited, ARC House, Terrace Road South, BinfIeld, RG42 4PZ.

Tel : 01344 397777 Fax : 01344 862010

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk) Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Plasterdrain.

* Stud height : 5mm.
* Colour : Clear.
* Fixing : Fix between studs.

- Fasteners : RIW Plaster Plugs.

- Fixing centres : Minimum : 13 number per square metre, in a diamond pattern.

- Sealing : RIW Sealing Rope around RIW Plaster Plugs before insertion.

* Joints : Minimum overlap ; 2 No studs. Provide row of fixings at overlap position.

- Sealing : RIW Overtape

- Drainage components : See Clauses 382 & 388. Control panels and alarms available.

* Accessories : RIW Cavity Drain Overtape ; see also product data sheet

RIW Cementseal Primer ; anti-lime treatment

WORKMANSHIP

J40/310 WORKMANSHIP GENERALLY

* Condition of substrate :

- Clean and even textured, free from voids and sharp protrusions.

- Moisture content : Compatible with damp proofing / tanking.

* Air and surface temperature : Do not apply sheets if below minimum recommended by
* Condition of membrane at completion :

- Neat, smooth and fully supported, dressed well into abutments and around intrusions.

- Completely impervious and continuous.

- Undamaged. Prevent puncturing during following work.

* Permanent overlying construction : Cover membrane as soon as possible.

J40/320 INSPECTION

* Give notice : Before covering any part of membrane with overlying construction.

J40/370 A PIPES, DUCTS, CABLES, ETC :

* Where these pass through sheeting, make junctions completely impervious, following details as recommended for the purpose by the sheet manufacturer.

J40/382 CAVITY DRAINAGE CHANNELS

* Manufacturer : RIW Limited, ARC House, Terrace Road South, Binfield, RG42 4PZ.

Tel : 01344 397777 Fax : 01344 862010

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk) Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Aqua Channel

J40/388 CAVITY DRAINAGE SUMPS WITH INTEGRAL PUMPS

* Manufacturer : RIW Limited, ARC House, Terrace Road South, Binfield, RG42 4PZ.

Tel : 01344 397777 Fax : 01344 862010

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk) Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Aqua Pump Pro + Battery back-up system

- Type : Manufacturer’s standard.

- Flow rate : Manufacturer’s standard.

- Pumping head (minimum) : Manufacturer’s standard.

- Discharge pipe size : Manufacturer’s standard.

or

- Product reference : RIW Aqua Pump Pro plus

- Type : Manufacturer’s standard.

- Flow rate : Manufacturer’s standard.

- Pumping head (minimum) : Manufacturer’s standard.

- Discharge pipe size : Manufacturer’s standard.

or

- Product reference : RIW Aqua Pump Pro

- Type : Manufacturer’s standard.

- Flow rate : Manufacturer’s standard.

- Pumping head (minimum) : Manufacturer’s standard.

- Discharge pipe size : Manufacturer’s standard.