J40 APPLIED TANKING / DAMP PROOFING

To be read with Preliminaries / General conditions.

**EXECUTION continued.**

J30/361 JUNCTIONS WITH STRUCTURESEAL

* RIW Sheetseal 226 to be overlapped by 150mm onto the applied RIW Structureseal.
* Seal together using 50 x 5mm bead of RIW Sealing Compound, in centre of lap.
* Apply remaining RIW Sheetseal 226, as required, in accordance with J40 /190

.