E40 DESIGNED JOINTS IN INSITU CONCRETE

To be read with Preliminaries / General conditions.

J40/310333333333

3100110101010293I8E4844444

320 HYDROPHILIC WATERSTOPS

- Manufacturer : RIW Ltd, 487/488 Ipswich Road, Slough, Berkshire SL1 4EQ

Tel : +44 1753 944200

E-mail : [technical@riw.co.uk](mailto:technical@riw.co.uk)

Web : [www.riw.co.uk](http://www.riw.co.uk)

- Product reference : RIW Waterstop

- Location : Fixed to the first cast concrete surface, centrally in 150mm minimum thickness of concrete.

* Method of fixing : Tightly butt joint the Waterstop as required. Do not overlap. Fix the RIW Waterstop in place using RIW Mesh ( lapped as necessary ), nailed through the Waterstop, at 300mm centres.
* Condition of concrete surface at time of fixing : Clean and free from ponded or running water.
* Protection : Prevent wetting of exposed sections of Waterstop.